PRISM LiDAR Cloud — Survey CAD Deliverable
====================================================
Horizontal datum : NAD83(2011) / Maryland (ftUS) (EPSG:6488)
Vertical datum   : NAVD88 (GEOID18, rigorous per-cell undulation (bilinear))
  geoid undulation N across AOI: +32.003 to +32.022 m (+104.997 to +105.060 ftUS) (added: H = h + N)
Units            : US survey feet  [US survey foot (1200/3937 m = 0.3048006096012192 m)]
Coordinate basis : GRID (state-plane grid coordinates)
Combined factor  : 0.99994300  (grid_to_ground; ground = grid / factor)  @ lon/lat -77.06226,38.91165
  grid scale 0.99995004 x elevation factor 0.99999296
----------------------------------------------------
DRAFT — PRISM LiDAR Cloud is an automated mapping tool, NOT a sealed survey. This deliverable is unsigned, PRISM-derived data; certification as a survey of record is the responsibility of a licensed Professional Surveyor & Mapper under the statutes of the deliverable's jurisdiction. North arrow, scale, bearing basis (Grid North, SPCS/NOS), control description, and positional accuracy are to be completed and sealed by the PSM.
----------------------------------------------------
PRISM·lidarcloud — provenance
Engine      : PRISM·lidarcloud v5_4_10
Integration : 6.0.0-dev
Run         : job
Input       : epsg26985
Epsg        : 26985
Modules:
  bench.classification       1.0.0
  bench.dep3                 1.0.0
  bench.dep3_aggregate       1.0.0
  bench.dep3_sample          1.0.0
  bench.dep3_score           1.0.0
  bench.isprs                1.0.0
  breakline.detect           1.0.0
  breakline.vectorize        1.0.0
  cad                        1.0.0
  cad.crs                    1.0.0
  cad.dxf                    1.0.0
  cad.landxml                1.2.0
  cad.pipeline               1.2.0
  cad.stamp                  1.2.0
  cad.surface                1.0.0
  cad.vertical               1.0.0
  change.core                1.1.0
  color                      1.2.1
  color.awss3                1.0.0
  color.cog                  1.0.0-dev
  color.consistency          1.1.0
  color.drape                1.0.0
  color.fusion               1.0.0-dev
  color.laswrite             1.0.0
  color.mosaic               1.0.0
  color.raster               1.6.1
  color.reflectance          1.0.0
  color.registration         1.0.0
  color.rgbtiff              1.0.0-dev
  color.selection            1.0.0
  color.sources              1.2.0
  color.stac                 1.0.0-dev
  export                     1.2.0
  hydro.watermask            1.0.0
  ign.fetch_lidarhd_urban    1.0.0
  report.density             1.1.0
  report.docx                1.5.0
  report.facts               1.4.0
  report.fgdc                1.3.0
  report.narrate             1.1.1
  report.pdf                 1.11.0
  report.units               1.0.0
  stats.robust               1.0.0
  survey.geoid               1.1.0
  usgs.ept                   1.0.0
  validate.adjust            1.2.0
  validate.asprs             1.1.0
  validate.checkpoints       1.3.1
  validate.coregister        1.0.0
  validate.demdiff           1.0.0
  validate.dep3raster        1.0.0
  validate.epqs              1.1.1
  vector.extent              1.0.0
  vector.io                  1.0.0

Files:
  dxf: PRISM_topo.dxf
  landxml: PRISM_surface.xml

counts: contours=705 spots=1521 tin_faces=710472
warnings:
  - TIN decimated x2 (1425348 valid cells > 1000000 cap)